For 1990-2009 cars

### Relief Procedure

#### Tools Required

J 34730-1A Fuel Pressure Gauge

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Connect J 34730-1A fuel pressure gauge to the fuel pressure connection. In order to avoid spillage, wrap a shop towel around the fuel pressure connection while connecting the fuel pressure gauge .
3. Install the bleed hose into an approved container and open the valve to bleed the system pressure. The fuel connections are now safe for servicing.
4. Drain any fuel remaining in the fuel pressure gauge into an approved container.