For 1990-2009 cars

### Removal Procedure

1. Remove the carpet retainers. Refer to Front Carpet Retainer Replacement , and Rear Carpet Retainer Replacement .
2. Pull out the door weatherstrip, if necessary.
3. Use a flat-bladed tool disengage the retaining clips for the pillar lower trim panel (1).
4. Remove the trim panel from the center pillar.

### Installation Procedure

1. Align the trim panel (1) to center pillar.
2. Press the trim panel (1) into the center pillar to engage the retaining clips.
3. Install the carpet retainers. Refer to Front Carpet Retainer Replacement , and Rear Carpet Retainer Replacement .
4. Install the door weatherstrips, if necessary.