For 1990-2009 cars

### Removal Procedure

1. Relieve fuel system pressure. Refer to Fuel Pressure Relief Procedure .
2. Drain the fuel tank. Refer to Fuel Tank Draining .
3. Remove the fuel tank. Refer to Fuel Tank Replacement .
4. Remove the modular fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
5. Remove the fuel level sensor from the modular fuel sender.

### Installation Procedure

1. Install the fuel level sensor to modular fuel sender.
2. Install the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
3. Install the fuel tank. Refer to Fuel Tank Replacement .
4. Refill the fuel tank.
5. Connect the negative battery cable.
6. Inspect for fuel leaks through the following steps:

6.1. | Turn the ignition switch to the ON position for two seconds

6.2. | Turn the ignition switch to the OFF position for ten seconds.

6.3. | Turn the ignition switch to the ON position

6.4. | Check for fuel leaks.