For 1990-2009 cars

#### Tools Required

J 28467-360 Engine Support Fixture

### Removal Procedure

1. Remove cruise control module from bracket and position aside. Refer to Cruise Control Module Replacement in Cruise Control.
2. Install the J 28467-360 and raise the engine off of the mount.
3. Remove the nuts attaching the mount to the body.
4. Remove the bolts (1) attaching the engine mount to the bracket.
5. Remove the engine mount (2).

### Installation Procedure

1. Install the engine mount (2).
2. Install the bolts (1) attaching the engine mount to the bracket. Do NOT tighten.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the nuts attaching the mount to the body.

Tighten

• | Tighten the engine mount to bracket bolts to 130 N·m (96 lb ft).

• | Tighten the engine mount nuts to 66 N·m(49 lb ft).

4. Remove the J 28467-360 .
5. Install cruise control module. Refer to Cruise Control Module Replacement in Cruise Control.