For 1990-2009 cars

1. Visually inspect the adjuster actuator spring (2) for the following:

• | Excessive corrosion

• | Excessive stretching

• | Broken hook ends

• | Twisting or binding

• | Missing

2. If any of the conditions listed were found, the drum brake system adjuster hardware requires replacement.
3. Visually inspect the adjuster actuator lever (1) for the following conditions:

• | Bent

• | Broken

• | Missing

• | Broken spring attachment tab

4. If any of the conditions listed were found, the adjuster actuator lever and/or attaching hardware requires replacement.