For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Squeeze the oblong connector at the following locations in order to disconnect the cables:

• | The motors (6, 7)

• | The vertical/horizontal actuators (3, 13)

### Installation Procedure

1. Connect the cables (1) by pushing onto the connector until you hear a click.
2. Install the front seat. Refer to Front Seat Replacement - Bucket .