For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the push-in retainers (3) from the rear bumper energy absorber.
3. Remove the rear bumper energy absorber (2) from the impact bar (1).

### Installation Procedure

1. Position the rear bumper energy absorber (2) to the impact bar (1).
2. Install the push-in retainers (3) to the rear bumper energy absorber (3).
3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .