For 1990-2009 cars

### Removal Procedure

Caution: To help avoid personal injury or damage to the vehicle, a bent, cracked, or damaged fan blade or housing should always be replaced.

1. Remove the cooling fan. Refer to Engine Cooling Fan Replacement .
2. Remove the fan nuts (9) from the fans (1, 8).
3. Remove the fans (1, 8) from the fan motors (3, 7).
4. Remove the fan motor bolts (2) from the fan motors (3, 7).
5. Remove the fan motors (3, 7).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the fan motor bolts (2) to the fan motors (3, 7).

Tighten
Tighten the bolts to 6 N·m (53 lb in).

2. Install the fans (1, 8) to the fan motors (3, 7).
3. Install the fan nuts (9) to the fans (1, 8).

Tighten
Tighten the nut to 6 N·m (53 lb in).

4. Install the cooling fan. Refer to Engine Cooling Fan Replacement .