For 1990-2009 cars

### Removal Procedure

1. Remove the seat adjuster covers (2), if equipped. The covers snap onto the seat adjusters in the front and rear.
2. Position the front seat assembly forward in order to gain access to the seat adjuster attaching bolts.
3. Remove the seat adjuster attaching bolts.
4. Remove the seat belt wire harness (driver's side only).
5. Disconnect the power seat electrical connector, if equipped (driver's side only).
6. Remove the front seat. Manually tilt the seat forward in order to disengage the hooks from the floor pan.

### Installation Procedure

1. Install the front seat. Manually tilt the seat forward in order to engage the hooks onto the floor pan.
2. Connect the power seat electrical connector, if equipped (driver's side only).
3. Install the seat belt wire harness (driver's side only).
4. Position the front seat assembly forward in order to gain access to the seat adjuster attaching bolts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the seat adjuster bolts.

Tighten
Tighten the seat adjuster bolt to 40 N·m (30 lb ft).

6. Install the adjuster covers (2), if equipped.