For 1990-2009 cars

1. Turn the steering wheel so that the vehicle's wheels are pointing straight ahead.
2. Turn OFF the ignition.
3. Remove the key from the ignition switch.
4. Remove the LH I/P wiring harness junction block.access panel
5. Remove the AIR BAG Fuse from the LH I/P wiring harness junction block.

Important: With the AIR BAG Fuse removed and the ignition ON, the AIR BAG warning lamp illuminates. This is a normal operation and does not indicate an SIR system malfunction.

6. Remove the connector position assurance (CPA) (2) from the driver yellow 2-way connector (1) located above the LH I/P wiring harness junction block.
7. Disconnect the driver yellow 2-way connector (1).
8. Remove the RH I/P wiring harness junction block.access panel
9. Remove the connector position assurance (CPA) (2) from the passenger yellow 2-way connector (3) located above the RH I/P wiring harness junction block.
10. Disconnect the passenger yellow 2-way connector (3).