For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank filler door screws (2).
2. Remove the fuel tank filler door (1) from the vehicle.
3. Remove the gas cap tether from the fuel tank filler door.

### Installation Procedure

1. Position the fuel tank filler door (1) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the fuel tank filler door screws (2).

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the gas cap tether to the fuel tank filler door.