For 1990-2009 cars

#### Tools Required

J 37043 Parking Brake Cable Release Tool

### Removal Procedure

1. Remove the center console. Refer to Front Floor Console Replacement in Instrument Panel, Gages and Console.
2. Remove the carpet from the left side of the vehicle. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
3. Remove the parking brake cable (2) from the parking brake lever reel (1).
4. Disconnect the cable from the parking brake lever using the J 37043 .
5. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
6. Remove the front parking brake cable (5) at the equalizer (3).
7. Disconnect the front parking brake cable mounting bracket (1).
8. Remove the front cable from the vehicle.

### Installation Procedure

1. Install the front cable into the vehicle.
2. Connect the front parking brake cable mounting bracket (1).
3. Connect the front parking brake cable (5) at the equalizer (3).
4. Lower the vehicle.
5. Connect the cable (2) to the parking brake lever.
6. Install the carpet to the left side of the vehicle. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
7. Install the center console. Refer to Front Floor Console Replacement in Instrument Panel, Gages and Console.
8. Adjust the parking brake. Refer to Park Brake Adjustment .