For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Untie the drawstrings (1) from the cover.
3. Remove the hog ring retainers (3).
4. Remove the cover (2) from the pad. The hook and loop strips retain the cover onto the pad.

### Installation Procedure

1. Install the cover (2) onto the pad.
2. Pull the draw strings (1).
3. Attach the drawstring hooks to the openings in the seat frame.
4. Install the hog ring retainers (3).