For 1990-2009 cars

## Door Lock Switch Replacement Oldsmobile

### Removal Procedure

1. Perform the following steps in order to remove the left-hand door power lock switch:

1.1. | Pry under the front or rear of the power lock and window switch bezel. Use a flat-bladed screwdriver in order to disengage the spring clips, and pull the switch free.

1.2. | Disconnect the electrical connectors.

2. Perform the following steps in order to remove the right-hand door power lock switch:

2.1. | Pry under the front or rear of the power lock and window switch. Use a flat-bladed screwdriver in order to disengage the spring clips, and pull the switch free.

2.2. | Disconnect the electrical connectors.

### Installation Procedure

1. Perform the following steps in order to install the left-hand door power lock switch:

1.1. | Connect the electrical connector.

1.2. | Install the door power lock to the bezel switch.

1.3. | Install the power lock and window switch bezel.

2. Perform the following steps in order to install the right-hand door power lock switch:

2.1. | Connect the connector.

2.2. | Install the door power lock switch to the bezel.

2.3. | Install the power lock and window switch bezel.

## Door Lock Switch Replacement Pontiac

### Removal Procedure

1. Position the power door lock bezel assembly (1) to the left front side of the door trim panel. Apply inboard pressure to the bezel's rear retaining clip in order to remove the bezel assembly.
2. Disconnect the power door lock connector (2) from the wire harness. Apply sufficient pressure in order to disengage the lock tab.

### Installation Procedure

1. Engage the power door lock connector (1) to the wire harness. Apply sufficient pressure to engage the lock tab.
2. Position the power door lock bezel assembly (2) to the left front side of the trim panel. Apply inboard pressure to the bezel rear retaining clip in order to instal the bezel assembly.