For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cable to Solenoid Nut | 12 N·m | 106 lb in
Flywheel Inspection Cover Bolt | 10 N·m | 89 lb in
Generator Bolt/Stud | 50 N·m | 37 lb ft
Generator Bracket Bolt | 50 N·m | 37 lb ft
Generator Nut (3.4 L) | 30 N·m | 22 lb ft
Negative Battery Cable Bolt | 15 N·m | 11 lb ft
Positive Battery Cable Bolt | 15 N·m | 11 lb ft
Solenoid Battery Terminal Nut | 9.5 N·m | 84 lb in
Solenoid S Terminal Nut | 2.5 N·m | 22 lb in
Starter Bolt (2.4 L) | 90 N·m | 66 lb ft
Starter Bolt (3.4 L) | 43 N·m | 32 lb ft