For 1990-2009 cars

1. Lubricate the tilt spring.
2. Install the tilt spring guide to the tilt spring.

Caution: The tilt spring and the spring guide are under pressure. The tilt spring and the spring guide may become a projectile. Secure the spring with locking pliers during removal. Secure the spring with locking pliers during installation. Bodily injury may result during removal and installation of the tilt spring and the spring guide. Always use caution during removal and installation of the tilt spring and the spring guide.

3. Install the tilt spring (1) to the post on the steering column support assembly.
4. Secure the tilt spring (1) with locking pliers by performing the following steps:

4.1. | While the end of the tilt spring is on the post, pull the center of the tilt spring (1) while pushing the tilt spring guide end to the post on the bearing and housing assembly.

4.2. | With both ends installed on the post, push the tilt spring into position.