For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat to rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.
2. Disconnect the amplifier wiring harness connector.
3. Remove the radio speaker amplifier bracket (2) bolts from the rear window trim panel.
4. Lower the amplifier bracket (2) from the rear parcel shelf.
5. Remove the four amplifier bolts.
6. Remove the amplifier (1) from the bracket (2).

### Installation Procedure

1. Install the amplifier (1) to the bracket (2).
2. Install the four amplifier bolts until fully seated and not stripped.
3. Raise the amplifier bracket (2) into the mounting position.
4. Install the bracket bolts to the rear window trim panel.
5. Connect the amplifier wiring harness connector.
6. Install the rear seat to rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.