For 1990-2009 cars

#### Tools Required

• | J 29569-1 Turbine Shaft Seal Installer

• | J 29569-2 Turbine Shaft Seal Sizer

• | J 29829-1 Turbine Shaft Seal Installer

• | J 29829-2 Turbine Shaft Seal Sizer

1. Assemble the drive sprocket (37) onto the turbine shaft (39).
2. Retain the drive sprocket with the turbine shaft to drive sprocket snap ring (35).
3. In order to assemble three new Teflon seals (33, 40) onto the turbine shaft (39), perform the following procedure:

3.1. | Slide the J 29569-1 over the large spline of the turbine shaft.

3.2. | Coat the J 29569-1 with transmission fluid.

3.3. | Use your fingers in order to guide the new Teflon™ seals over the J 29569-1 and into the seal ring grooves on the turbine shaft.

3.4. | Remove the J 29569-1 when the seals are in place.

| Important: In order to properly size the seals, keep the J 29569-2 in place for 5 minutes.

3.5. | Size the new Teflon™ seals. Use both halves of the J 29569-2 .

3.6. | Repeat steps 3.1 through 3.6 with J 29829-1 and J 29829-2 on the small splined side of the turbine shaft.