For 1990-2009 cars

### Removal Procedure

Caution: The seat belt assembly and/or bracket assembly must be replaced as a unit only. Do not substitute parts for any reason, or personal injury could result.

Important: Replace the anchor bracket if the anchor bracket is damaged.

1. Remove the bolts (1).
2. Remove the anchor bracket (3).

### Installation Procedure

1. Connect the anchor bracket (3) to the anchor bracket mounting plate.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: DO NOT use a nut driver to tighten this hardware or the fasteners will not be properly seated.

2. Install the tether anchor bolts.

Tighten
Tighten the tether anchor bolts to 20 N·m (15 lb ft).