For 1990-2009 cars

### Removal Procedure

1. Remove the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
2. Pull out the door weatherstrips as required.
3. Remove the shoulder belt bolt. Refer to Seat Belt Retractor Replacement - Left Front in Seat Belts.
4. Use a flat-bladed tool to remove the center pillar upper trim panel (1) from its clips.

### Installation Procedure

1. Position the center pillar upper trim panel (1) to align the retaining clips.
2. Press in to secure the retaining clips.
3. Install the shoulder belt bolt. Refer to Seat Belt Retractor Replacement - Left Front in Seat Belts.
4. Install the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
5. Install the door weatherstrips.