For 1990-2009 cars

### Removal Procedure

1. Lower the front door window.
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Pull up on the front door inner belt sealing strip (1) in order to release the strip from the clips.

### Installation Procedure

1. Position the inner sealing strip tabs to the pinchweld (1) on the inner door frame.
2. Install the inner sealing strip, by pressing into place until fully seated.
3. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .