For 1990-2009 cars

Range | Park/ Neutral | Reverse | D | 3 | 2 | 1
--- | --- | --- | --- | --- | --- | ---
Gear | N | R | 1st | 2nd | 3rd | 4th | 1st | 2nd | 3rd | 1st | 2nd | 3rd** | 1st | 2nd***
1-2 Shift Solenoid | ON | ON | ON | OFF | OFF | ON | ON | OFF | OFF | ON | OFF | OFF | ON | OFF
2-3 Shift Solenoid | OFF | OFF | OFF | OFF | ON | ON | OFF | OFF | ON | OFF | OFF | ON | OFF | OFF
2nd Clutch | -- | -- | -- | A | A* | A* | -- | A | A* | -- | A | A* | -- | A
2nd Roller Clutch | -- | -- | -- | H | O | -- | -- | H | O | -- | H | O | -- | H
Int./4th Band | -- | -- | -- | -- | -- | A | -- | -- | -- | -- | A | -- | -- | A
Reverse Clutch | -- | A | -- | -- | -- | -- | -- | -- | -- | -- | -- | -- | -- | --
Coast Clutch | -- | -- | -- | -- | -- | -- | A | A | A | A | A | A | A | A
Input Sprag | -- | -- | H | H | H | O | H | H | H | H | H | H | H | H
Direct Clutch | -- | -- | -- | -- | A | A | -- | -- | A | -- | -- | A | -- | --
Forward Clutch | -- | -- | A | A | A | A* | A | A | A | A | A | A | A | A
Lo/Rev Band | A | A | -- | -- | -- | -- | -- | -- | -- | -- | -- | -- | A | --
Lo Roller Clutch | -- | -- | H | O | O | O | H | O | O | H | O | O | H | O

- A = Applied
- H = Holding
- O = Overrunning
- ON = The solenoid is energized
- OFF = The solenoid is de-energized
- * = Applied with no load
- ** = Manual SECOND-THIRD gear is only available above approximately 100 km/h (62 mph)
- *** = Manual FIRST-SECOND gear is only available above approximately 60 km/h (37 mph)
- Manual FIRST-THIRD gear is also possible at high vehicle speed as a safety feature