For 1990-2009 cars

## Side Window Defogger Outlet Duct Replacement - Left Side Oldsmobile

### Removal Procedure

1. Remove the I/P trim pad. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gages, and Console.
2. Remove the left defogger outlet duct retainer from the air distribution duct.
3. Remove the left defogger outlet duct retainer from the HVAC module assembly.
4. Remove the left defogger outlet duct from the vehicle.

### Installation Procedure

1. Install the left defogger outlet duct over the air distribution duct.
2. Install the left defogger outlet duct retainer to the air distribution duct.
3. Install the left defogger outlet duct retainer to the HVAC module assembly.
4. Install the I/P trim pad. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gages, and Console.

## Side Window Defogger Outlet Duct Replacement - Left Side Pontiac

### Removal Procedure

1. Remove the I/P trim pad. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gages, and Console.
2. Remove the left defogger outlet duct retainer from the air distribution duct.
3. Remove the left defogger outlet duct from between the crush bracket.

### Installation Procedure

1. Install the left defogger outlet duct through the crush bracket and under the air distribution duct.
2. Install the left defogger outlet duct retainer to the air distribution duct.
3. Install the I/P trim pad. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gages, and Console.