For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Firmly pull the lower quarter trim panel away from the vehicle in order to release the retainers.
3. Remove the panel from the vehicle.

### Installation Procedure

1. Install the panel to the vehicle.
2. Press firmly against the panel. Ensure that the fasteners are locked into position.
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .