For 1990-2009 cars

### Removal Procedure

1. Position the front to the most rearward position.
2. Remove the EZ entry release handle retaining clips.
3. Remove the EZ entry release handle from the seat track studs.

### Installation Procedure

1. Install the EZ entry release handle to the seat track studs.
2. Install the EZ entry release handle retaining clips, pressing into place until fully seated.
3. Position the front to the original position.