For 1990-2009 cars

### Circuit Description

The Low Traction indicator is controlled by the instrument cluster via serial data messages from the EBCM. When the ABS or TCS is active for 0.5 seconds, the EBCM commands the instrument cluster to turn ON the Low Traction indicator.

The Low Traction indicator will also turn ON during the instrument cluster bulb check. When the ignition switch is turned to ON, the Low Traction indicator will turn ON for approximately 3 seconds and then turn OFF.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. Use the scan tool to check the normal state of the Low Traction indicator control.

2. Ensures that the instrument cluster can operate the Low Traction indicator.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Antilock Brake System Schematics Connector End View Reference: Antilock Brake System Connector End Views or Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gages, and Console
1 | Did you perform the ABS Diagnostic System Check? | Go to Step 2 | Go to Diagnostic System Check - ABS
2 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.
3. With a scan tool, observe the ETS Active Lamp parameter in the ETS data list.

Does the scan tool display Off?

Go to Step 3

Go to Step 4

3 |

1. Turn OFF the ignition.
2. Turn ON the ignition, with the engine OFF.
3. Observe the Low Traction indicator on the instrument cluster (IPC) during the bulb check.

Does the Low Traction indicator illuminate during the bulb check and then turn OFF?

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

Go to Step 5

4 | Inspect for poor connections at the harness connector of the EBCM. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 8 | Go to Step 6
5 | Inspect for poor connections at the harness connector of the instrument cluster (IPC). Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 8 | Go to Step 7
6 | Replace the EBCM. Refer to Electronic Brake Control Module Replacement . Did you complete the repair? | Go to Step 8 | --
7 | Replace the instrument cluster (IPC). Refer to Instrument Cluster Replacement in Instrument Panel, Gages and Console. Did you complete the repair? | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2