For 1990-2009 cars

### Removal Procedure

1. Remove the intermediate shaft. Refer to Intermediate Steering Shaft Replacement .
2. Remove the intermediate shaft seal (1).

### Installation Procedure

Caution: If steering column to cowl panel seal is torn or otherwise damaged, it must be replaced. Confirm that the seal and inner race are properly located. Failure to do so may allow carbon monoxide into the vehicle, which may result in serious personal injury or death.

1. Install the intermediate shaft seal (1).
2. Install the intermediate shaft. Refer to Intermediate Steering Shaft Replacement .