For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Untie and loosen the drawstrings from the rear seat cushion cover.
3. Unhook the rear seat cover loops from the rear seat frame tabs.
4. Unhook the rear seat cover loops from the rear seat frame tabs.
5. Pull back the rear seat cushion cover from the pad.
6. Reach inside of the rear seat cover in order to unfasten the hook and the loop retainers securing the rear seat back cover to the pad.
7. Remove the rear seat cushion cover from the pad.

### Installation Procedure

1. Install the rear seat cushion cover onto the pad.
2. Hook the rear seat cover loops to the rear seat frame tabs.
3. Use firm hand pressure in order to fasten the hook and the loop retainers, securing the rear seat back cover to the pad.
4. Pull the draw string tight.
5. Attach the draw string to the last tab on the seat frame and tie off.
6. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .