For 1990-2009 cars

### Removal Procedure

The rear floor heat duct is located under the console and floor carpeting.

1. Remove the console. Refer to Console Replacement Instrument Panel, Gauges and Console.
2. Partially remove the floor carpeting to the rear of the front seat. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
3. Remove the rear floor duct (3).

### Installation Procedure

1. Install the rear floor duct (3).
2. Install the floor carpeting.
3. Install the console.