For 1990-2009 cars

### Removal Procedure

1. Remove the front seats. Refer to Front Seat Replacement - Bucket in Seats.
2. Remove the console assembly. Refer to Front Floor Console Replacement in Instrument Panel, Gages, and Console.
3. Remove the front door carpet retainer. Refer to Front Carpet Retainer Replacement
4. Remove the rear door carpet retainer. Refer to Rear Carpet Retainer Replacement .
5. Remove the front shoulder belt anchor bolts from the floor pan. Refer to Seat Belt Retractor Replacement - Left Front or to Seat Belt Retractor Replacement - Right Front in Seat Belts.
6. Remove the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
7. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
8. Remove the floor carpet.

### Installation Procedure

Caution: In order to avoid personal injury or vehicle damage when you repair or replace the carpet, use the same thickness and material size as the original installation. Always return the carpet to the original location.

1. Position the floor carpet.
2. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .
3. Install the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
4. Install the front shoulder belt anchor bolts to the floor pan. Refer to Seat Belt Retractor Replacement - Left Front or to Seat Belt Retractor Replacement - Right Front in Seat Belts.
5. Install the rear door carpet retainers. Refer to Front Carpet Retainer Replacement .
6. Install the front door carpet retainer. Refer to Front Carpet Retainer Replacement .
7. Install the console assembly. Refer to Front Floor Console Replacement in Instrument Panel, Gages, and Console.
8. Install the front seats. Refer to Front Seat Replacement - Bucket .