For 1990-2009 cars

## DTC P0730 2.2 L and 3.4 L

### Circuit Description

The PCM calculates gear ratio based on the transmission input and output speeds. The PCM compares the known transmission gear ratio to the calculated ratio for the selected gear range.

When the PCM detects an unknown transmission gear ratio, then DTC P0730 sets. DTC P0730 is a type C DTC.

### Conditions for Running the DTC

• | No TP sensor DTCs P0121, P0122, or P0123.

• | No VSS DTCs P0502 or P0503.

• | No AT ISS DTCs P0716 or P0717.

• | No TFP manual valve position switch DTC P1810.

• | The engine is running.

• | The TFP manual valve position switch is not indicating PARK or NEUTRAL.

• | The time since the gear select lever change is greater than 6 seconds.

• | The transmission fluid temperature is greater than 20°C (68°F).

• | The TP is greater than 15 percent.

• | The vehicle speed is greater than 8 km/h (5 mph).

### Conditions for Setting the DTC

One of the following conditions occurs for 7 seconds:

• | The gear ratio is greater than 3.13:1.

• | The gear ratio is 2.23:1 to 2.87:1.

• | The gear ratio is 1.71:1 to 2.02:1.

• | The gear ratio is 1.07:1 to 1.54:1.

• | The gear ratio is 0.72:1 to 0.91:1.

• | The gear ratio is less than 0.61:1.

### Action Taken When the DTC Sets

• | The PCM does not illuminate the malfunction indicator lamp (MIL).

• | The PCM commands maximum line pressure.

• | The PCM freezes transmission adapt functions.

• | The PCM records the operating conditions when the Conditions for Setting the DTC are met. The PCM stores this information as Failure Records.

• | The PCM stores DTC P0730 in PCM history.

### Conditions for Clearing the DTC

• | A scan tool can clear the DTC.

• | The PCM clears the DTC from PCM history if the vehicle completes 40 warm-up cycles without a non-emission-related diagnostic fault occurring.

• | The PCM cancels the DTC default actions when the ignition switch is OFF long enough in order to power down the PCM.

### Diagnostic Aids

• | Inspect for intermittent automatic transmission input, shaft, speed sensor (AT ISS) circuit conditions.

• | Inspect for intermittent automatic transmission output, shaft, speed sensor (AT OSS) circuit conditions.

• | Inspect for an incorrect calibration.

• | Refer to Range Reference .

• | Ensure the wiring harness is not stretched too tightly or other components are pressing on the connector body. Also, inspect for proper clearance to any other components and wiring. Refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step tests for low fluid level, which may cause slipping, and result in an incorrect gear ratio.

2. This step verifies that the correct gear ratios occur for commanded gears.

3. This step tests for low line pressure.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain Diagnostic System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Engine Controls in Engine Controls - 2.2 L or Diagnostic System Check - Engine Controls in Engine Controls - 3.4 L
2 |

1. Visually inspect the transmission cooling system for fluid leaks.
2. Repair any leaks as necessary.

Refer to Fluid Leak Diagnosis .

Did you find and correct a condition?

--

Go to Step 8

Go to Step 3

3 | Did you perform the Transmission Fluid Checking Procedure? | -- | Go to Step 4 | Go to Transmission Fluid Check
4 |

1. Install a Scan Tool .
2. Turn ON the ignition, with the engine OFF.

Important: Before clearing the DTC, use the Scan Tool in order to record the Failure Records. Using the Clear Info function erases the Failure Records from the PCM.

3. Record the DTC Failure Records.
4. Clear the DTC.
5. Use the Scan Tool snapshot mode in order to record the transmission gear ratios.
6. Drive the vehicle in transmission gear ranges 1, 2, 3, and D with the TP greater than 15%, and the vehicle speed greater than 8 km/h (5 mph).
7. Record each transmission gear.

Did the gear ratio match the specified ranges?

Reverse: 2.02:1-2.23:1

1st: 2.87:1-3.13:1

2nd: 1.54:1-1.71:1

3rd: 0.91:1-1.07:1

4th: 0.61:1-0.72:1

Go to Diagnostic Aids

Go to Step 5

5 | Did you perform the Line Pressure Check Procedure? | -- | Go to Step 6 | Go to Line Pressure Check
6 |

1. Inspect for excessive clutch wear.

Refer to Clutch Plate Diagnosis .

2. Repair as necessary.

Refer to Transmission Overhaul in Transmission Unit Repair Manual.

Did you complete the repair?

--

Go to Step 7

--

7 |

1. Change the AT fluid and filter.

Refer to Automatic Transmission Fluid Filter and Seal Replacement .

2. Inspect the transmission fluid for correct level.
3. Add new fluid as necessary.

Important: The Clear TAPS function will clear all adapt cells. This may affect transmission performance. The PCM will update the adapt cell values as the vehicle is driven.

4. Use the Scan Tool in order to perform the Clear TAPS function.

Did you complete the above procedures?

--

Go to Step 8

--

8 | Perform the following procedure in order to verify the repair:

1. Select DTC.
2. Select Clear Info.
3. Operate the vehicle under the following conditions:

• | Drive the vehicle with the throttle greater than 15% in order to obtain any one of the following gear ratios for 7 seconds.

• | Reverse: 2.02:1-2.23:1

• | 1st: 2.87:1-3.13:1

• | 2nd: 1.54:1-1.71:1

• | 3rd: 0.91:1-1.07:1

• | 4th: 0.61:1-0.72:1

4. Select Specific DTC.
5. Enter DTC P0730.

Has the test run and passed?

--

System OK

Go to Step 1