For 1990-2009 cars

### Removal Procedure

1. Remove the front seat back. Refer to Front Seat Back Replacement .
2. Remove the head rest. Refer to Front Seat Head Restraint Replacement .
3. Remove the head rest guides. Refer to Front Seat Head Restraint Replacement .
4. Remove the cover (1) from the pad/frame assembly (2).

### Installation Procedure

1. Install the cover (1) onto the pad/frame assembly (2).
2. Install the head rest guides. Refer to Front Seat Head Restraint Replacement .
3. Install the head rest. Refer to Front Seat Head Restraint Replacement .
4. Install the front seat back. Refer to Front Seat Back Replacement .