For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

### Removal Procedure

1. Open the hood.
2. Remove the wiper arm assemblies. Refer to Windshield Wiper Arm Replacement in Wipers/Washer Systems.
3. Disconnect the washer tubing from the air inlet screen.
4. Using J 38778 , remove the air inlet grille panel push-in retainers (1) from the panel.
5. Remove the air inlet grille panel from the vehicle.

### Installation Procedure

1. Position the air inlet grille panel to the vehicle.
2. Install the air inlet grille panel push-in retainers (1) to the panel.
3. Connect the washer tubing to the air inlet panel.
4. Install the wiper arms and blade assemblies. Refer to Windshield Wiper Arm Replacement in Wipers/Washer Systems.
5. Close the hood.