For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Power Window Schematics
1 | Did you perform the Diagnostic System Check for the door systems? | Go to Step 2 | Go to Diagnostic System Check - Door Systems
2 | Verify that the passenger window lockout function does not work properly. Does the lockout function operate properly? | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems | Go to Step 3
3 |

1. Disconnect the driver window switch.
2. Test the lockout signal circuit of the power window master switch for an open, for a short to voltage, or for a short to ground. Refer to Circuit Testing and to Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

Go to Step 5

Go to Step 4

4 | Replace the driver window switch. Refer to Front Side Door Window Switch Replacement - Left Side . Is the repair complete? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2