For 1990-2009 cars

Repair the rear defogger bus bars or reattach the terminals by soldering using a solder containing the following ingredients:

• | Silver -- 3%

• | Lead -- 27%

• | Tin 70 -- 27%

• | A rosin flux paste

1. Before soldering the bus bar, buff the repair area using a fine steel wool. This removes the oxide coating that forms during the rear window manufacture.
2. Apply a paste-type rosin flux in small quantities to the terminal and/or bus bar repair area using a brush.
3. Ensure that the soldering iron tip is coated with solder beforehand. Use only enough heat to melt the solder and enough solder to ensure a complete repair.
4. Do not overheat the terminal when soldering.