For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the screws from the instrument panel cluster.
3. Remove the instrument cluster from the instrument panel.
4. Disconnect the electrical connector from the instrument panel.

### Installation Procedure

1. Connect the electrical connector to the instrument panel cluster.
2. Position the instrument cluster to the instrument panel alignment tabs.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screws to the instrument panel cluster.

Tighten
Tighten the instrument panel console screws to 2 N·m (18 lb in).

4. Install the instrument panel cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .