For 1990-2009 cars

### Removal Procedure

1. Remove the sunshade from the sunshade anchor.
2. Remove the bezel screws.
3. Disconnect the electrical connector, if equipped.
4. Remove the sunshade.

### Installation Procedure

1. Position the sunshade.
2. Connect the electrical connector, if equipped.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the bezel screws.

Tighten
Tighten the screws to 1.9 N·m (17 lb in).

4. Place the sunshade in the anchor.