For 1990-2009 cars

Problem | Action
--- | ---
A misaligned column |

1. Inspect the following components:

• | The column

• | Verify that the alignment is correct.

• | The mounting

• | The bearings

2. Adjust , repair and/or replace the components as needed.

Refer to Steering Column Replacement

A deformed or improperly installed shaft seal |

1. Inspect for proper installation.
2. Reseat the seal.
3. Tighten the seal to specifications.
4. Replace the seal as needed.

Refer to Intermediate Steering Shaft Seal Replacement

A tight intermediate shaft universal joint | Clean, inspect and replace as needed. Refer to Intermediate Steering Shaft Replacement