For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint to Steering Knuckle Nut | 55 N·m | 41 lb ft
Control Arm to Frame Bolts (Front Bushing) | 60 N·m plus 180 degree rotation | 45 lb ft
Control Arm to Frame Bolts (Rear Vertical Bushing) | 100 N·m plus 180 degree rotation | 74 lb ft
Hub and Bearing to Steering Knuckle Bolts | 95 N·m | 70 lb ft
Stabilizer Shaft Clamp | 66 N·m | 49 lb ft
Stabilizer Shaft Link Nuts | 17 N·m | 13 lb ft
Strut Assembly to Body Bolt | 25 N·m | 18 lb ft
Strut Assembly to Body Nuts | 25 N·m | 18 lb ft
Strut to Steering Knuckle Nuts | 180 N·m | 133 lb ft
Strut Nut to Strut Rod | 75 N·m | 55 lb ft
Suspension Crossmember Bolts | 110 N·m | 81 lb ft
Transmission Mount Bolt | 120 N·m | 89 lb ft