For 1990-2009 cars

## Steering Wheel Control Switches Replacement Pontiac

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the steering wheel control switch(s) from the steering wheel pad using a small flat-bladed tool.
3. Disconnect the electrical connector from the steering wheel control switch(s).
4. Remove the steering wheel control switch(s) from the steering wheel.

### Installation Procedure

1. Connect the electrical connector to the steering wheel control switch.
2. Position the steering wheel control switch(s) to the steering wheel pad.
3. Install the steering wheel control switch(s) to the steering wheel pad pressing into place until fully seated.
4. Inspect the operation of the steering wheel control switch(s).
5. Enable the SIR system. Refer to Enabling the SIR System in SIR.

## Steering Wheel Control Switches Replacement Oldsmobile

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.
3. Remove the screws from the steering wheel control switch.
4. Remove the steering wheel control switch from the steering wheel.
5. Disconnect the electrical connector from the steering wheel control switch.

### Installation Procedure

1. Connect the electrical connector to the steering wheel control switch.
2. Position the steering wheel control switch to the steering wheel.
3. Install the screws to the steering wheel control switch.

Tighten
Tighten the steering wheel control switch screws to 2 N·m (19 lb in).

4. Inspect the operation of the steering wheel control switch.
5. Install the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.
6. Enable the SIR system. Refer to Enabling the SIR System in SIR.