For 1990-2009 cars

### Diagnostic Aids

Important: Perform the following in order to avoid misdiagnosis.

• | Inspect for proper operation of brake lamps.

• | Inspect throttle linkage for mechanical binding which could cause the system to malfunction.

• | Inspect cruise control cable adjustment, should have minimum slack.

• | When testing vehicles with steering wheel controls, the steering wheel must be rotated to each stop position while testing the cruise control switch signal circuits. This will assure the integrity of the SRI coil.

• | EMI on the speed sensor signal circuit may cause erratic cruise control operation.

### Conditions for Enabling Cruise Control

• | When vehicle speed is more than 40 km/h (25 mph)

• | When PARK, REVERSE, NEUTRAL, or 1st gear is not indicated.

• | When an over/undercharged battery condition does not exist.

• | With normal engine RPM.

• | Without high engine RPM (fuel cut-off).

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: Cruise Control Schematics
1 | Did you perform A Diagnostic System Check - Cruise Control ? | -- | Go to Step 2 | Go to Diagnostic System Check - Cruise Control
2 |

1. Turn OFF the ignition.
2. Disconnect the cruise control module.
3. Turn ON the ignition, with the engine OFF.
4. Probe the ignition positive voltage circuit of the cruise control module with a test lamp that is connected to a good ground.

Does the test lamp illuminate?

--

Go to Step 3

Go to Step 40

3 | Probe the ignition positive voltage circuit of the cruise control module with a test lamp that is connected to the ground circuit of the cruise control module. Does the test lamp illuminate? | -- | Go to Step 4 | Go to Step 41
4 |

1. Turn ON the ignition, with the engine OFF.
2. Turn OFF the cruise control.
3. Probe the cruise control on switch signal, the set/coast switch, and the resume/accelerate switch signal circuits with a test lamp that is connected to a good ground.

Does the test lamp illuminate on any of the signal circuits?

--

Go to Step 18

Go to Step 5

5 |

1. Turn ON the ignition, with the engine OFF.
2. Turn ON the cruise control switch.
3. Probe the cruise control on switch signal circuit with a test lamp that is connected to a good ground.

Does the test lamp illuminate?

--

Go to Step 6

Go to Step 19

6 |

1. Probe the cruise control set/coast switch signal circuit with a test lamp that is connected to a good ground.
2. Press and hold the SET/COAST button.

Does the test lamp illuminate?

--

Go to Step 7

Go to Step 21

7 |

1. Probe the cruise control resume/accelerate switch signal circuit with a test lamp that is connected to a good ground.
2. Press and hold the RESUME/ACCEL switch.

Does the test lamp illuminate?

--

Go to Step 8

Go to Step 22

8 | Probe the cruise control release signal circuit with a test lamp that is connected to a good ground. Does the test lamp illuminate? | -- | Go to Step 9 | Go to Step 23
9 | Press the brake pedal while monitoring the test lamp. Does the test lamp illuminate? | -- | Go to Step 24 | Go to Step 10
10 | Probe the stop lamp signal circuit with a test lamp that is connected to a good ground. Does the test lamp illuminate? | -- | Go to Step 25 | Go to Step 11
11 | Press the brake pedal while monitoring the test lamp. Does the test lamp illuminate? | -- | Go to Step 12 | Go to Step 26
12 | Probe the cruise control inhibit signal circuit with a test lamp that is connected to B+. Does the test lamp illuminate? | -- | Go to Step 29 | Go to Step 13
13 | Use a scan tool in order to command the cruise inhibit/enable OFF. Does the test lamp illuminate? | -- | Go to Step 14 | Go to Step 30
14 | Probe the cruise control engaged signal circuit with a DMM that is connected to a good ground. Does the voltage measure near the specified value? | B+ | Go to Step 15 | Go to Step 31
15 | Important: If equipped with a cancel switch (Oldsmobile) use steps 15, 16. Vehicles with out cancel switch go to step 17.

1. Turn OFF the ignition.
2. Disconnect the appropriate BCM harness connector.
3. Turn ON the ignition, with the engine OFF.
4. Probe the cruise control cancel signal circuit with a test lamp connected to a good ground.

Does the test lamp illuminate?

--

Go to Step 16

Go to Step 27

16 | Press the cruise control cancel switch while monitoring the test lamp. Does the test lamp illuminate? | -- | Go to Step 28 | Go to Step 17
17 | Check the speedometer for proper operation. Does the speedometer operate properly? | -- | Go to Step 32 | Go to Symptoms - Instrument Cluster
18 | Test the signal circuit that illuminated the test lamp for a short to voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 34
19 | Test the cruise control on switch signal circuit for an open or a high resistance and the set/coast and resume/accel signal circuits for a short to ground.. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 20
20 | Test the ignition positive voltage circuit for an open or high resistance between the IP junction block and the cruise control switch. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 38
21 | Test the cruise control set/coast signal circuit for an open or a high resistance. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 38
22 | Test the cruise control resume/accelerate signal circuit for an open or a high resistance. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 38
23 | Test the cruise control release switch signal circuit for an open or a high resistance. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 33
24 | Test the cruise control release switch signal circuit for a short to voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 33
25 | Test the stoplamp switch signal circuit for a short to voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 34
26 | Test the stoplamp switch signal circuit for an open or a high resistance. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 34
27 | Test the cruise control cancel circuit for an open or high resistance. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 38
28 | Test the cruise control cancel circuit for a short to voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 38
29 | Test the cruise inhibit signal circuit for a short to ground. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 37
30 | Test the cruise inhibit signal circuit for an open, a high resistance, or a short to voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 37
31 | Test the cruise engaged signal circuit for an open, a high resistance, or a short to voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 37
32 | Test the speed sensor circuit for an open or a high resistance between the PCM and cruise control module. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 39
33 | Inspect the cruise control release switch for proper adjustment. Refer to Brake Release Switch Adjustment. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 35
34 | Inspect the stoplamp switch for proper adjustment. Refer to Stop Lamp Switch Adjustment. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 36
35 | Inspect for poor connections at the harness connector of the cruise control release switch. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 42
36 | Inspect for poor connections at the harness connector of the stoplamp switch. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 43
37 | Inspect for poor connections at the harness connector of the PCM. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 44
38 | Inspect for poor connections at the harness connector of the cruise control switch. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairsin Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 45
39 | Inspect for poor connections at the harness connector of the cruise control module. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairsin Wiring Systems. Did you find and correct the condition? | -- | Go to Step 47 | Go to Step 46
40 | Repair the ignition positive voltage circuit of the cruise control module. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Step 47 | --
41 | Repair the ground circuit of the cruise control module. Refer to Wiring Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Step 47 | --
42 | Replace the cruise control release switch. Refer to Brake Release Switch Replacement. Did you complete the replacement? | -- | Go to Step 47 | --
43 | Replace the stop lamp switch. Refer to Stop Lamp Switch Replacement in Hydraulic Brakes. Did you complete the replacement? | -- | Go to Step 47 | --
44 | Replace the PCM. Refer to Powertrain Control Module Replacement/Programming 2.4L or Powertrain Control Module Replacement/Programming 3.4L in Engine Controls. Did you complete the replacement? | -- | Go to Step 47 | --
45 | Replace the cruise control switch. Refer to Cruise Control Switch Replacement. Did you complete the replacement? | -- | Go to Step 47 | --
46 | Replace the cruise control module. Refer to Cruise Control Module Replacement. Did you complete the replacement? | -- | Go to Step 47 | --
47 | Operate the vehicle within the conditions for cruise control operation. Does the cruise control system operate correctly? | -- | System OK | Go to Step 2