For 1990-2009 cars

### Removal Procedure

Remove the rear compartment lid weather-strip (1) from the gutter flange.

### Installation Procedure

Important: Apply light hand pressure in order to seat the strip when installing the rear compartment lid weather-strip to the flange. Heavy impacting, such as with a mallet, will result in waterleaks.

1. Install the rear compartment lid weather-strip (1) to the gutter flange.
2. Inspect the entire flange opening in order to ensure that the clinch is completely seated.
3. Use a hose with no nozzle attached in order to test the weather-strip for leaks.
4. If leaks are present, perform the following steps:

4.1. | Remove the weather-strip.

4.2. | Brush the weather-strip adhesive, P/N 3M-08011 or the equivalent, around the perimeter of the flange.

4.3. | Install and retest the weather-stripping for leaks.