For 1990-2009 cars

#### Tools Required

J 41101 Pass-Through Connector Remover

1. Push the J 41101 or equivalent onto the pass-through connector from the outside of the transmission case in order to compress the pass-through connector's retaining tabs.
2. With the retaining tabs compressed, use a screwdriver in order to remove the pass-through connector through the inside of the transmission case.
3. Remove the wiring harness (11).