For 1990-2009 cars

### Removal Procedure

1. Remove the trim plate from the instrument panel cluster. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
2. Disconnect the electrical connector from the trip odometer and reset switch.
3. Release the retainers on the trip odometer and reset switch by using a small flat-bladed tool.
4. Remove the trip odometer and reset switch from the trim plate.

### Installation Procedure

1. Align the trip odometer and reset switch to the trim plate.
2. Install the trip odometer and reset switch by pressing into place until fully seated.
3. Connect the electrical connector to the trip odometer and reset switch.
4. Install the trim plate to the instrument panel cluster. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .