For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
3. Remove the transmission oil filter assembly. Refer to Automatic Transmission Fluid Filter and Seal Replacement .
4. Remove the 4 forward clutch and the lo and reverse band oil bolts that attach the oil feed pipe assembly to the transmission.
5. Remove the lo and the reverse band oil pipe assembly.
6. Remove the 8 lo and the reverse band oil pipe assembly seals.
7. Inspect the oil feed pipes for plugged passages, bent pipes, or cracks.
8. Check the oil feed pipe seal rings. Verify the proper location of the seal rings. Replace the seal rings if these are cut, swelled or damaged.

### Installation Procedure

1. Use Mercon® IIl Automatic Transmission Fluid in order to lube and install the 8 lo and the reverse band oil pipe assembly seals.
2. Install the lo and the reverse band oil feed pipe assembly onto the transmission.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Hand start the 4 forward clutch and the lo and the reverse band oil bolts that attach the oil feed pipe assembly to the transmission.

Tighten
Tighten the bolts to 12 N·m (106 lb in).

4. Install the transmission oil pan and gasket. Refer to Automatic Transmission Fluid Filter and Seal Replacement .
5. Lower the vehicle.
6. Refill the transmission to the proper level. Refer to Transmission Fluid Check .