For 1990-2009 cars

### Removal Procedure

1. Remove the left instrument panel sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gages and Console.
2. Disconnect the accelerator cable from the accelerator pedal.
3. Squeeze the accelerator cable cover tangs and push the accelerator cable through the bulkhead.
4. Remove the accelerator cable shield, if equipped.
5. Disconnect the accelerator cable from the retaining clips.
6. Disconnect the accelerator cable from the throttle body lever.
7. Disconnect the accelerator cable from the accelerator cable bracket.
8. Remove the accelerator cable from the vehicle noting cable routing.

### Installation Procedure

Notice: Do not route flexible components (hoses, wires, conduits, etc.) within 50 mm (2 in) of moving parts unless flexible components can be securely fastened. This is necessary in order to prevent possible interference and damage to the component.

1. Reinstall accelerator cable into car using routing noted during removal.
2. Snap the cable retainer through the bulkhead.
3. Connect the accelerator cable through the slot in the accelerator pedal lever.
4. Seat the snap retainer in the accelerator pedal lever.
5. Connect the accelerator cable to the throttle body lever.
6. Connect the accelerator cable to the accelerator cable bracket.
7. Connect the accelerator cable into the retaining clips.
8. Reinstall the accelerator cable shield, if equipped.
9. Reinspect and check for complete throttle opening and closing positions by operating the accelerator pedal. Also check for poor carpet fit under the accelerator pedal.
10. Reinspect the throttle should operate freely, without binding, between full closed and wide open throttle.
11. Reinstall the left instrument panel sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gages and Console.