For 1990-2009 cars

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement in Automatic Transaxle - 4T40-E/4T45-E.
2. Remove the flywheel. Refer to Engine Flywheel Replacement .
3. Remove the crankshaft rear oil seal. Refer to Crankshaft Rear Oil Seal Removal .

### Installation Procedure

1. Install the rear main seal. Refer to Crankshaft Rear Oil Seal Installation .
2. Install the flywheel. Refer to Engine Flywheel Replacement .
3. Install the transmission. Refer to Transmission Replacement in Automatic Transaxle - 4T40-E/4T45-E.
4. Inspect for proper fluid levels.
5. Inspect for leaks.