For 1990-2009 cars

### Modes of Operation

#### Automatic Door Locks (Manual Trans)

The following are the modes of operation for the automatic door locks feature:

• | Mode 1:

| All of the doors lock when the vehicle speed exceeds 8 km/h (5 mph). All of the doors will unlock when the transaxle is shifted into REVERSE (R) and the key is turned to OFF.

| Mode 2: if equipped with RKE

| All of the doors lock when the vehicle speed exceeds 8 km/h (5 mph). Only the driver door unlocks when the transaxle is shifted into REVERSE (R) the key is turned to OFF.

• | Mode 3:

| All of the doors lock when the vehicle speed exceeds 8 km/h (5 mph). No automatic door unlock.

• | Mode 4:

| No automatic door lock or unlock.

#### Automatic Door Locks (Automatic Trans)

The following are the modes of operation for the automatic door locks feature:

• | Mode 1:

| All of the doors lock when the vehicle is shifted out of PARK. All of the doors unlock when the vehicle is shifted into PARK and the key is turned to OFF.

• | Mode 2:

| All of the doors lock when the vehicle is shifted out of PARK. Only the driver door unlocks when the vehicle is shifted into PARK and the key is turned to OFF.

• | Mode 3:

| All of the doors lock when the vehicle is shifted out of PARK. No automatic door unlock.

• | Mode 4:

| The automatic door lock feature is disabled.

### Programming Features

#### Enter Programming

To enter the programming mode, perform the following actions:

1. On a vehicle with a manual trans, place the trans in REVERSE. Apply the park brake.
2. Close all of the doors.
3. Turn the ignition to the RUN position.

#### Automatic Door Locks

Continue with the following steps in order to personalize the automatic door locks:

1. Press hold the LOCK button on the power door lock switch for 10 seconds. The vehicle will chime with the number of chimes corresponding to the current mode. Refer to Automatic Door Locks modes.
2. Press and hold the LOCK button on the power door lock switch for 10 seconds again in order to advance to the next mode. The vehicle will chime with the number of chimes corresponding to the mode.
3. Continue to press and hold the LOCK button on the transmitter until the desired mode is reached.

#### Remote Activation Verification

Continue with the following steps in order to personalize the horn for the remote activation verification feature:

1. Press and hold the power door lock switch in the UNLOCK position for 10 seconds. The horn will chirp when the horn setting for the remote activation verification has changed between disable and enable.
2. Press and hold the power door lock switch in the UNLOCK position for 10 seconds again to change the horn setting back to the original setting. The horn will chirp when the horn setting for the remote activation verification has changed.

#### Exit Programming

Any of the following list of events will cause the programming sequence to be terminated:

• | The ignition is moved from the RUN position.

• | The vehicle is shifted out of REVERSE for vehicles with a manual trans.

• | The park brake is released for vehicles with a manual trans.

### Chime Level Adjustment

In order to adjust the chime level, perform the following steps:

1. Turn the ignition ON.
2. Turn the radio OFF.
3. Press and hold the radio push-button 6 until either LOUD or NORMAL appears on the radio display. The chime sounds 3 times for each volume change.
4. To toggle the setting, press and hold the radio push-button 6 again.

### Additional Information

For more information on the personalization features, refer to one of the following description and operations:

• | Refer to Power Door Locks Description and Operation in Doors for more information about the automatic door lock feature.

• | Refer to Keyless Entry System Description and Operation in Keyless Entry for more information about the remote activation verification feature.

• | Refer to Theft Systems Description and Operation in Theft Deterrent for more information about the Content Theft Deterrent feature.

• | Refer to Audible Warnings Description and Operation in Instrument Panel, Gauges and Console for more information about the Chime.