For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat back. Refer to Rear Seat Back Replacement
2. Pull the seat back pad cover over the upper loops of the seat frame.
3. Pull the upper draw string over the T-hooks.
4. Remove the seat back cover from the T-hooks.
5. Remove the seat back cover from the seat frame U-brackets.
6. Remove the seat back cover from the pad.
7. Reach inside seat back cover and unfasten the hook and the loop retainers from the pad.
8. Remove the cover from the lower seat frame loops.
9. Pull the lower draw string over the seat frame U-brackets
10. Remove the seat back cover from the pad.

### Installation Procedure

1. Install the seat back pad cover to the lower seat frame loops.
2. Install the seat back cover to the pad.
3. Align the hook and the loop retainers.
4. Use firm pressure to fasten the hook and the loop retainers.
5. Align the two bottom openings for the seat back cover with the U-brackets.
6. Install the seat back cover so that the U-brackets at the bottom are through the opening in the cover.
7. Install the top of the seat back cover to the T-hooks.
8. Install the seat back pad cover to the seat frame upper loops.
9. Pull the upper draw string over the T-hooks.
10. Install the seat back. Refer to Rear Seat Back Replacement .