For 1990-2009 cars

## Defroster Grille Replacement Pontiac

### Removal Procedure

1. Release the defroster grille retainers from the instrument panel (IP) using a small flat-bladed tool.
2. Remove the defroster grille from the IP by pulling up and out.

### Installation Procedure

1. Position the defroster grille to the IP.
2. Install the defroster grille to the IP. Press the grille into place until fully seated.